|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Date | Equipment Checked | Result of Calibration Pass/ Fail | Corrective Action | Checked By |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
| \*\*\*Thermometers should be checked at least annually must be accurate to within +1ºC or -1ºC\*\*\* | | | | |