|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Date  | Equipment Checked  | Result of Calibration Pass/ Fail  | Corrective Action  | Checked By  |
|   |   |   |   |   |
|   |   |   |   |   |
|   |   |   |   |   |
|   |   |   |   |   |
|   |   |   |   |   |
|   |   |   |   |   |
|   |   |   |   |   |
|   |   |   |   |   |
|   |   |   |   |   |
|   |   |   |   |   |
|   |   |   |   |   |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|   |   |   |   |   |
|   |   |   |   |   |
|   |   |   |   |   |
|   |   |   |   |   |
| \*\*\*Thermometers should be checked at least annually must be accurate to within +1ºC or -1ºC\*\*\* |